|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Item | Part Name | Material Type | Dimensions | Stand. / Code /Spec | Qty | Weight | Material | Note(s) |
| 1 | SUPPORT | PLATE | 344 X 140 | NOT APPLICABLE | 02 | 7,2 | SA-240 316/L |  |
| 2 | ARM | PIPE | Ø3” SCH. 80 x 1590 | NOT APPLICABLE | 01 | 23,7 | SA-312 TP316/L |  |
| 3 | HANDLE | ROUND BAR | Ø38 x 35 | NOT APPLICABLE | 01 | 0,3 | SA-276 316/L |  |
| 4 | HANDLE BAR | ROUND BAR | Ø5/8” x 230 | NOT APPLICABLE | 01 | 0,4 | SA-276 316/L |  |
| 5 | WASHER | WASHER | M16 | DIN 125 A | 01 | 0,1 | SS 316/L |  |
| 6 | LUG | PLATE | 110 x 100 x 1/2” | NOT APPLICABLE | 01 | 1,1 | SA-240 316/L |  |
| 7 | PIN | ROUND BAR | Ø1 1/2" x 75 | NOT APPLICABLE | 01 | 0,7 | SA-276 316/L |  |
| 8 | SPLIT PIN | PIN | Ø3,7 x 40 | DIN 94 / ISO 1234 | 01 | 0,1 | SS 316/L |  |
| 9 | RETAINING RING | RETAINING RING | Ø38 | DIN 471 | 02 | 0,1 | SS 316/L |  |
| 10 | THREADED ROD | THEADED ROD | M16 x 405 | ISO 68-1 | 01 | 0,6 | SA-193 B7 |  |
| 11 | STOP | PLATE | Ø110 x 89 x 1/2" | NOT APPLICABLE | 01 | 0,3 | SA-240 316/L |  |
| 12 | WASHER | PLATE | Ø110 x 92 x 1/2" | NOT APPLICABLE | 01 | 0,3 | SA-240 316/L |  |
| 13 | SLEEVE | PIPE | Ø3 1/2" SCH. 10 x 229 | NOT APPLICABLE | 01 | 1,6 | SA-312 TP316/L |  |
| 14 | CLOSURE | PLATE | Ø72 x 1/2" | NOT APPLICABLE | 02 | 0,4 | SA-240 316/L |  |

Notes:

1. Total weight: 44,6 kg
2. Dimensions in **millimeter**, weight in **kilogram**.
3. Dual certification for the stainless material allowed

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Rev. | Description | Date | Created by | Reviewed by | Approved by |
| 1 | Fist issue | 01.12.24 | John Edward | Satoshi Ihiro | Joshua Nobilibe |
| 2 |  |  |  |  |  |
| 3 |  |  |  |  |  |